AJA-FS3-MIB DEFINITIONS ::= BEGIN

--
-- MIB objects for FS3 Implementation
--

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, 
    Integer32,
    NOTIFICATION-TYPE           FROM SNMPv2-SMI
    
	TEXTUAL-CONVENTION, DisplayString,
	TruthValue, DateAndTime, AutonomousType   FROM SNMPv2-TC
	
	fs3Product		FROM AJA-ROOT-MIB
;

fs3MIB MODULE-IDENTITY
    LAST-UPDATED "201401210000Z"
    ORGANIZATION "AJA Video Systems Inc."
    CONTACT-INFO    
	 "postal:   John Abt
                P.O. Box 1033
                Grass Valley CA  95945

          email:    ianaadmin@aja.com
          webpage:  www.aja.com"
    DESCRIPTION
	"This module defines snmp data and notifications in the FS3 product"
    REVISION     "201401210000Z"
    DESCRIPTION
	"Initial release"
    ::= { fs3Product 50 } 

--
-- top level structure
--

fs3Scalars       OBJECT IDENTIFIER       ::= { fs3MIB 1 }
fs3Alarms        OBJECT IDENTIFIER       ::= { fs3MIB 2 }

fs3Integer OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
	"This is a simple object which merely houses a writable
	 integer.  It's only purposes is to hold the value of a single
	 integer.  Writing to it will simply change the value for
	 subsequent GET/GETNEXT/GETBULK retrievals.

	 This example object is implemented in the
	 agent/mibgroup/examples/scalar_int.c file."
    DEFVAL { 42 }
    ::= { fs3Scalars 1 }

--
-- Alarm objects
--

fs3PowerSupply1Alarm OBJECT-TYPE
    SYNTAX      OCTET-STRING
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "FS3 power supply 1 Alarm."
    DEFVAL { "Unknown State; default" }
::= { fs3Alarms 2 }

fs3PowerSupply2Alarm OBJECT-TYPE
    SYNTAX      OCTET-STRING
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "FS3 power supply 2 Alarm."
    DEFVAL { "Unknown State; default" }
::= { fs3Alarms 3 }

fs3ReferenceAlarm OBJECT-TYPE
    SYNTAX      OCTET-STRING
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Reference Alarm."
    DEFVAL { "Unknown State; default" }
::= { fs3Alarms 4 }

--
-- Vid1 Reference Alarm may not be used but is here for completeness
-- fs3ReferenceAlarm will alarm if any Genlock source fails 
-- (beit "Reference", "Vid1 Input")
--
fs3Vid1ReferenceAlarm OBJECT-TYPE
    SYNTAX      OCTET-STRING
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Video Proc 1 Reference Alarm."
    DEFVAL { "Unknown State; default" }
::= { fs3Alarms 5 }

--
-- Video Proc 1 format alarms
--
fs3Vid1FormatAlarm OBJECT-TYPE
    SYNTAX      OCTET-STRING
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Format incompatibility Video Proc 1 Alarm."
    DEFVAL { "Unknown State; default" }
::= { fs3Alarms 7 }


--
-- Over Temp
--
fs3OverTemperatureAlarm OBJECT-TYPE
    SYNTAX      OCTET-STRING
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Over Temp Range Alarm."
    DEFVAL { "Unknown State; default" }
::= { fs3Alarms 11 }



END
