AJA-FS2-MIB DEFINITIONS ::= BEGIN

--
-- MIB objects for FS2 Implementation
--

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, 
    Integer32,
    NOTIFICATION-TYPE           FROM SNMPv2-SMI
    
	TEXTUAL-CONVENTION, DisplayString,
	TruthValue, DateAndTime, AutonomousType   FROM SNMPv2-TC
	
	fs2Product		FROM AJA-ROOT-MIB
;

fs2MIB MODULE-IDENTITY
    LAST-UPDATED "201103170000Z"
    ORGANIZATION "AJA Video Systems Inc."
    CONTACT-INFO    
	 "postal:   Fred Dominikus
                P.O. Box 1033
                Grass Valley CA  95945

          email:    ianaadmin@aja.com
          webpage:  www.aja.com"
    DESCRIPTION
	"This module defines snmp data and notifications in the FS2 product"
    REVISION     "201103170000Z"
    DESCRIPTION
	"Initial release"
    ::= { fs2Product 30 } 

--
-- top level structure
--

fs2Scalars       OBJECT IDENTIFIER       ::= { fs2MIB 1 }
fs2Alarms        OBJECT IDENTIFIER       ::= { fs2MIB 2 }

fs2Integer OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
	"This is a simple object which merely houses a writable
	 integer.  It's only purposes is to hold the value of a single
	 integer.  Writing to it will simply change the value for
	 subsequent GET/GETNEXT/GETBULK retrievals.

	 This example object is implemented in the
	 agent/mibgroup/examples/scalar_int.c file."
    DEFVAL { 42 }
    ::= { fs2Scalars 1 }

--
-- Alarm objects
--

fs2PowerSupply1Alarm OBJECT-TYPE
    SYNTAX      OCTET-STRING
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "FS2 power supply Alarm."
    DEFVAL { "Unknown State; default" }
::= { fs2Alarms 2 }

fs2PowerSupply2Alarm OBJECT-TYPE
    SYNTAX      OCTET-STRING
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "FS2 power supply Alarm."
    DEFVAL { "Unknown State; default" }
::= { fs2Alarms 3 }

fs2ReferenceAlarm OBJECT-TYPE
    SYNTAX      OCTET-STRING
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Reference Alarm."
    DEFVAL { "Unknown State; default" }
::= { fs2Alarms 4 }

--
-- Vid1 and 2 Reference Alarms may not be used but are here for completeness
-- fs2ReferenceAlarm will alarm if any Genlock source fails 
-- (beit "Reference", "Vid1 Input", "Vid2 Input")
--
fs2Vid1ReferenceAlarm OBJECT-TYPE
    SYNTAX      OCTET-STRING
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Video Proc 1 Reference Alarm."
    DEFVAL { "Unknown State; default" }
::= { fs2Alarms 5 }

fs2Vid2ReferenceAlarm OBJECT-TYPE
    SYNTAX      OCTET-STRING
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Video Proc 2 Reference Alarm."
    DEFVAL { "Unknown State; default" }
::= { fs2Alarms 6 }

--
-- Video Proc 1 format alarms
--
fs2Vid1FormatAlarm OBJECT-TYPE
    SYNTAX      OCTET-STRING
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Format incompatability Video Proc 1 Alarm."
    DEFVAL { "Unknown State; default" }
::= { fs2Alarms 7 }

fs2Vid1BackgroundAlarm OBJECT-TYPE
    SYNTAX      OCTET-STRING
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Video Proc 1 Background format Alarm."
    DEFVAL { "Unknown State; default" }
::= { fs2Alarms 8 }

--
-- Video Proc 2 format alarms
--
fs2Vid2FormatAlarm OBJECT-TYPE
    SYNTAX      OCTET-STRING
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Format incompatability Video Proc 2 Alarm."
    DEFVAL { "Unknown State; default" }
::= { fs2Alarms 9 }

fs2Vid2BackgroundAlarm OBJECT-TYPE
    SYNTAX      OCTET-STRING
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Video Proc 2 Background format Alarm."
    DEFVAL { "Unknown State; default" }
::= { fs2Alarms 10 }

--
-- Over Temp
--
fs2OverTemperatureAlarm OBJECT-TYPE
    SYNTAX      OCTET-STRING
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Over Temp Range Alarm."
    DEFVAL { "Unknown State; default" }
::= { fs2Alarms 11 }

--
-- fs2Audio1DolbyFramerAlarm
--
fs2Audio1DolbyFramerAlarm OBJECT-TYPE
    SYNTAX      OCTET-STRING
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Audio 1 Dolby Framer Alarm."
    DEFVAL { "Unknown State; default" }
::= { fs2Alarms 12 }

--
-- fs2Audio2DolbyFramerAlarm
--
fs2Audio2DolbyFramerAlarm OBJECT-TYPE
    SYNTAX      OCTET-STRING
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Audio 2 Dolby Framer Alarm."
    DEFVAL { "Unknown State; default" }
::= { fs2Alarms 13 }


END
