The driver must be installed with the Add New Hardware Wizard or the Update Hardware Wizard.
When you install a new board, the Add New Hardware Wizard should run automatically.

To invoke the Update Hardware Wizard in Windows XP, select Start > Control Panel >
 Administrative Tools > Computer Management > Device Manager > Sound, video, and game controllers >
 AJA Xena-SD Serial Digital Framestore > Driver > Update Driver.
